C   1997 GeoLogan97 Research Park Data in SEGY format 15July1997
C   Data: Integer*4  240byte header on each trace
C   Global Coord. Borehole: [x=0100.000  y=00100.000   z=1.0250 CE]
C   Local Coord: Ref (0., 2.17, 1.175)  Source: (0.00, 1.27, 1.025)
C   Tool Bowspring exits hole, R-component Azimuth=220 degrees
C
C Local Origin at (x,y)=(0,0), elevations above arbitrary datum, MKS units
C Elevation Not Surveyed.  North Well of deep pair
C       Local Origin at borhole NorthWell               New Source 135deg.
C       x-axis Azimuth=90deg=+ EAST   |-----------------------------------|
C       y-axis Azimuth=00deg=+ NORTH  | Geologic Log (Depth in meters)    |
C       z-axis Vertical=180deg=+ DOWN | (From CPT-3, ConeTech 11/01/96)   |
C                                     |  Location 200ft east (could be    |
C Instruments: Bison 9048 seismic data|  near boreholes, exact location   |
C Sample Interval = 0.00025seconds    |  unknown)                         |
C Record Length   = 0.5 seconds       |  00.0--06.7m  Clayey Silt and Clay|
C                                     |  06.7--18.6m  Sand                |
C Filters: Low Cut= 4 Hz              |  18.6--22.3m  Silt                |
C          High Cut=1000 Hz           |  22.3--25.6m  Silty sand          |
C NOTE: File 152 has Pile Driver Sig. |  25.6m        Gravel, Refusal     |
C                                     |-----------------------------------|
C 6 Channel Record:   OYO PHONE 14Hz     Water Table unknown              
C Sidewall Clamping Geophone (SWC)       NOTE: The several CPT soundings
C Ch1=Vertical Ch2=Radial Ch3=Transverse gave results similar to above.
C Reference Phone (REF)                  Files 1 to 146 normal VSP
C Ch4=Vertical Ch5=Radial Ch6=Transverse Files 147-150 source rotated
C   __________________________________________________________________
C   |                                                                |
C   | Processed By Dr. P. Michaels, PE                               |
C   |                                                                |
C   | Boise State University, Geosciences Department                 |
C   | Center for Geophysical Investigation of the Shallow Subsurface |
C   |________________________________________________________________|
C
C One shot record per data set including reel header
C  SEGY EXCEPTION: First break picks in header bytes      181-184 int*4
C                  Polarizations: Source azimuth=bytes    185-186 int*2
C                  (degrees)      Source vertical=bytes   189-190 int*2
C                                 Receiver azimuth=bytes  205-206 int*2
C                                 Receiver vertical=bytes 207-208 int*2
